Text for specification

Désignation
QUADRON^®Panel
support pour fusibles cylindriques
Class J / 3P, borne 150 mm²
200 A / 600 V (41x146)

Normes
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

Approbations
UL

Charactéristiques électriques

rated current (UL):	200 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	13,0 W

Icc:	200 kA

for Class J fuses 110 - 200A as per UL 248-8 (41x146)

Points de raccordement
AWG 2 - MCM 300 stranded, equivalent to 33,6 - 152mm²

Brand 
Woehner or equivalent

Référence
33409000