Text for specification

Désignation
transformateur de courant universel
pour montage dans le compartiment de raccordement
taille 1 - 3
185Power

Normes
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Charactéristiques électriques
Quadron®185Power Speed:
- max. 600 A
- increase of power dissipation by 30%

Quadron®185Power, connection bottom:
- max. 630 A
- increase of power dissipation by 35%

Crito®185Power connection rail, connection bottom:
- max. 750 A
- increase of power dissipation by 28% 

Brand 
Woehner or equivalent

Référence
33762000A