Text for specification

Désignation
profilé de cloisonnement
perforé
17 x 86 x 1100
60Classic

Normes
IEC 61439-1:2011

Charactéristiques électriques

Miscellaneous 
To safeguard against touching the busbars from above and below, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Référence
01041000