Text for specification

Désignation
rail de cuivre en lamelles, dénudé, isolé
5x 63 x 1
1061 A, longueur 2 m
Accessories

Normes
IEC 61439-1:2020

Approbations
UL

Charactéristiques électriques
Courant assigné (IEC):	1 061 A

power dissipation at full load of the item:	150,6 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Référence
01324000