Text for specification

Désignation
CAPUS^®Panel
interrupteur-sectionneur à 3 pôles
vis M10, poignée gris graphite
630 A

Normes
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approbations
IEC (CB)

Charactéristiques électriques
Courant assigné (IEC):	630 A
Tension assignée (IEC) CA:	500 V

AC-23B (500V)
AC-22B (500V)
AC-21B (500V)

power dissipation at full load of the item:	127,0 W

rated isolation voltage U_i AC:	1000 V
Tension assignée de tenue aux chocs Uimp:	12 kV
rated making capacity:	30 kA

Mechanical lifespan (switching operations) 7000
rated short-circuit making capacity 30kA

conv. therm. current in housing
630 A, horizontal installation (adjacent poles) encapsulated 504 x 378 x 302 mm
630 A, vertical installation (poles beneath each other) encapsulated 500 x 500 x 300 mm

Shock protection at front with terminal space cover IP40

Points de raccordement
vis M10 :
Md 25 - 31 Nm

Miscellaneous 
double-breaking main contacts, 
visible separation sections, 
user-independent switching, 
assembly and connection material contained in scope of delivery

Brand 
Woehner or equivalent

Référence
33335000