Text for specification

Désignation
MOTUS^®60Classic
démarreur moteur hybride 3 pôles
démareur direct inverse de 1,5 - 7,0 A / contacteur de charge résistive de 1,5 - 9,0 A
avec module IO-Link et technologie CrossLink®
60Classic

Normes
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-2:2011
IEC 61508-1:2010
ISO 13849-1:2015

Approbations
UL

Charactéristiques électriques
Courant assigné (IEC):	9 A
Tension assignée (IEC) CA:	500 V

rated current (UL):	7,6 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	12,0 W

rated isolation voltage U_i AC:	550 V
Tension assignée de tenue aux chocs Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 400 A / 600 V AC  

Points de raccordement
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Référence
36128000A