Text for specification

Descrizione
Vasca posteriore
290 x 1100
60Classic

Norme
IEC 61439-1:2011

Valori elettrici

Proprietà materiali
Copertura:
	resistenza alle temperature fino a 70°C, 
	ignifugo secondo UL 94

Miscellaneous 
To safeguard against touching the busbars from above, below and behind, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Cod. art.
01011000