Text for specification

Descrizione
Profilo di protezione
con feritoie
17 x 86 x 1100
60Classic

Norme
IEC 61439-1:2011

Valori elettrici

Miscellaneous 
To safeguard against touching the busbars from above and below, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Cod. art.
01041000