Text for specification

Descrizione
QUADRON®60Classic
Base per fusibili NH 250 A, collegam. in basso o in alto
morsetti a gabbia
Gr. NH 1 / 3P
60Classic

Norme
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Omologazioni
CCC

Valori elettrici
corrente nominale (IEC):	250 A
tensione nominale (IEC) AC:	690 V
tensione nominale (IEC) DC:	440 V

power dissipation at full load of the item:	31.4 W
tensione di picco Uimp:	6 kV
tensione max. ammissibile (IEC) AC:	800 V
tensione max. ammissibile (IEC) DC:	800 V
resistenza al corto circuito con protezione tramite fusibili:	80 kA

Adapter module, degree of protection IP20 at front

Connessioni
box terminal

Cu 70-185mm²f
Cu 35-150mm²s(r)
Cu 35-120mm²f+AE
lam.Cu 15.5-24mm large
terminal space 24.5 x 12mm
min. terminal space heigt 3mm

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
CrossLink® adapter technology
Fast and safe conversion of the connection for top or bottom
Simple and safe clicking into place and making contact
Safe connection through shock protection split into two
Busbar supports for flat busbars can be mounted above each other

Brand 
Woehner or equivalent

Cod. art.
03300000