Text for specification

Descrizione
SECUR®60Classic PowerLiner
sezionatore per fusibili D0, montaggio su barre
per fusibili D01 e D02, con LED
E18 / 63 A /3P
60Classic

Norme
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Omologazioni
VDE, CCC

Valori elettrici
corrente nominale (IEC):	63 A
tensione nominale (IEC) AC:	400 V
tensione nominale (IEC) DC:	110 V

AC-23A (400 V)

DC-21B (48V) 1 pole
DC-21B (110V) 2 poles

power dissipation at full load of the item:	10.5 W

tensione nominale di isolamento Ui AC:	500 V
tensione di picco Uimp:	6 kV

LED indicates blown fuse, operating range: 110 - 400 V AC / DC

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638: AC22

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

There is a transfer of the potential from the busbars, through the LED units, to the terminals  when the fuse links are removed and the switching mechanismn is closed. 

Brand 
Woehner or equivalent

Cod. art.
31525000