Text for specification

Descrizione
CRITO®60Classic
Piastra con morsetti di connessione, 3p
6 - 50 mm², AWG 10 - 2/0, lam. Cu. 7 - 9 x 4 - 10
60Classic

Norme
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Omologazioni
CSA, UL

Valori elettrici
corrente nominale (IEC):	175 A
tensione nominale (IEC) AC:	800 V

corrente nominale (UL):	175 A
tensione nominale (UL) AC:	600 V

power dissipation at full load of the item:	3,0 W
corrente d'impiego max. (IEC):	300 A
tensione di picco Uimp:	6 kV
tensione max. ammissibile (IEC) AC:	1000 V
tensione max. ammissibile (IEC) DC:	1500 V

resistenza nom. alla corrente di picco Ipk max.:	40,5 kA

SCCR: 65 kA with any DIVQ/7 circuit breaker 200 A / 480 V AC, 100 kA with JDDZ fuse Class J, CF or T 150 A / 600 V AC 

Connessioni
6 - 50 (70) mm² / AWG 10 - AWG 2/0 
cavi flessibili direttam. o con ferrula, 
cavi multifilari, 
bandelle flessibili 7x4 - 9x6
Md 8-10 Nm / 71 lb-in

(cavi flessibili con ferrula potrebbero no più entrare, se scelti con sezione max.  )

Proprietà materiali
Corpo base:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free
Copertura:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Miscellaneous 
Terminals can be removed for connection of uncut conductors

Brand 
Woehner or equivalent

Cod. art.
01240000