Text for specification

Descrizione
QUADRON®100Energy
Base verticale per fusibili NH00 160 A
morsetto a prisma 70 mm²
Gr. NH 00
100Energy

Norme
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Valori elettrici
corrente nominale (IEC):	160 A
tensione nominale (IEC) AC:	690 V

power dissipation at full load of the item:	17,5 W
tensione di picco Uimp:	6 kV
tensione max. ammissibile (IEC) AC:	800 V
resistenza al corto circuito con protezione tramite fusibili:	50 kA

Connessioni
wedge clamp terminal for Cu an Al:
stranded round 16 - 70 mm²,
stranded sectored 16 - 70 mm²,
flexible with wire-end ferrules 16 - 70 mm²

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Proprietà materiali
Corpo base:
	resistenza alle temperature fino a 125°C, 
	ignifugo secondo UL 94, 
	tenuta alle correnti di fuga CTI 200
Contatti:
	spring-loaded copper contacts, silver plated 
Protezione contro contatto accidentale:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
Undrilled mounting possible with terminal clamp

Brand 
Woehner or equivalent

Cod. art.
33384000