Text for specification

Descrizione
modulo universale per fissaggio TA
istallazione nella zona dei terminali
Gr. 1 - 3
185Power

Norme
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Valori elettrici
QUADRON®185Power Speed, connection top:
- max. 500 A
- increase of power dissipation by 16 %

QUADRON®185Power Speed, connection bottom:
- max. 600 A
- increase of power dissipation by 20 %

QUADRON®185Power, connection bottom:
- max. 600 A
- increase of power dissipation by 25 % 

Brand 
Woehner or equivalent

Cod. art.
33776000A