Text for specification

Descrizione
MOTUS®60Classic
avviatore ibrido, 3p
0,075 - 0,6 A avv. motore (avanti/indietro) / switch per carichi motore
60Classic

Norme
EN 60947-1:2015
EN 60947-4-2:2012
EN 61439-1:2012
EN 50581:2012
EN ISO 13849-1:2015

Omologazioni
UL, CCC

Valori elettrici
corrente nominale (IEC):	0,6 A
tensione nominale (IEC) AC:	500 V

corrente nominale (UL):	0,6 A
tensione nominale (UL) AC:	500 V

power dissipation at full load of the item:	2,8 W

tensione nominale di isolamento Ui AC:	500 V
tensione di picco Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 400 A / 600 V AC  

Connessioni
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Proprietà materiali
Involucro:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay
EMERGENCY STOP protection up to category 3

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Cod. art.
36102000B