Text for specification

Descrizione
barra a pettine, 3p, per 4 basi sezion.
35 mm²
Come accessorio

Norme
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Valori elettrici
power dissipation at full load of the item:	13,9 W

rated insulation voltage: 800V at pollution degree 2; 690V at pollution degree 3
For rated operating current, see download diagram

rated surge withstand capacity: 25 kA /400V;
rated short-time withstand current resistance: 12.5kA-100ms/400V

Degree of protection:
IP 20 at front in combination NH-LTS, comb-type busbar and connecting terminal possible.
Degree of protection near terminal depends on installation.

Miscellaneous 
Shock protection:	as per DIN EN 50274/BGV A3
Prefabricated for four NH- LTS closed version with end caps

Brand 
Woehner or equivalent

Cod. art.
33392000