Text for specification

Descrizione
CRITO®30Compact
Piastra con morsetti di connessione, 3p
35 - 150 mm², AWG 2 - 300 MCM,  lam. Cu. 15 - 20 x 5 - 10
30Compact 3P

Norme
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	275 A
tensione nominale (IEC) AC:	690 V

corrente nominale (UL):	285 A
tensione nominale (UL) AC:	600 V
corrente d'impiego max. (IEC):	480 A
tensione max. ammissibile (IEC) AC:	1000 V
tensione max. ammissibile (IEC) DC:	1500 V

resistenza nom. alla corrente di picco Ipk max.:	45,9 kA

SCCR:	18 kA

Connessioni
for applications acc. to IEC / EN :
35 - 150 mm² stranded round cables and stranded sectored cables
flexible cables, directly or with wire-end ferrule
(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

also for the connection of lam. Cu up to 20x10 

for applications acc. to UL / CSA :
only Cu cables Class B acc. to UL 486E
35 - 150 mm² / AWG 2 - MCM 300

Proprietà materiali
Corpo base:
	resistenza alle temperature fino a 125°C, 
	ignifugo secondo UL 94, 
	tenuta alle correnti di fuga CTI 200
Copertura:
	resistenza alle temperature fino a 125°C, 
	ignifugo secondo UL 94, 
	tenuta alle correnti di fuga CTI 200

Terminals: 	galvanised steel, chromited screw: 	hexagon socket screw M8 x 37, thrust piece: 	brass, nickel-plated

Miscellaneous 
Terminals with captive clamping screws
Conductor can be overlapped
Indication of nominal cross-section and tightening torque noted on the terminals.

Brand 
Woehner or equivalent

Cod. art.
01165000