Text for specification

Descrizione
QUADRON^®Panel
Base per fusibili NH 250 A, per pannello, per fotovoltaico
vite M10 a entrambi lati
Gr. NH 1XL / 1P, incl. protezione

Norme
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	250 A
tensione nominale (IEC) AC:	1000 V
tensione nominale (IEC) DC:	1500 V

corrente nominale (UL):	250 A
tensione nominale (UL) DC:	1500 V

power dissipation at full load of the item:	5,5 W
tensione di picco U_imp:	6 kV
resistenza al corto circuito con protezione tramite fusibili:	50 kA

SCCR:	15 kA

for fuse links IEC 60269-6

Proprietà materiali
Corpo base:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contatti:
	spring-loaded copper contacts, silver plated 
Viti di collegamento:
	screw M10, galvanized, chromized
Protezione contro contatto accidentale:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
For safe connection of the leads, the shock protection is split into 2.

Brand 
Woehner or equivalent

Cod. art.
03290000