Text for specification

Descrizione
Calotta terminali IP20 (frontale)
incl. 3 coperture sup.
larghezza 300mm
185Power

Norme
IEC 61439-1:2011

Valori elettrici

Proprietà materiali
Corpo base:
	temperature stability 125°C,
	self-extinguishing in acc. to UL 94,
	creepage resistance CTI 600,
	halogen-free
Copertura:
	temperature stability 125°C,
	fire behaviour UL 94 HB,
	creepage resistance CTI 200,
	halogen-free 

Brand 
Woehner or equivalent

Cod. art.
32700000A