Text for specification

Descrizione
Barra flessibile, rame stagnato, isolata
5x 40 x 1
736 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2011

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	736 A

power dissipation at full load of the item:	114,1 W

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Cod. art.
01097000