Text for specification

Descrizione
Barra con profilo TT, 500 mm²
lunghezza 3,60 m, stagnata
60Classic
185mm-System
centre feed unit

Norme
IEC 61439-1:2011

Omologazioni
CSA, UL

Valori elettrici
power dissipation at full load of the item:	240,0 W

diagram current capacity (IEC) 

Proprietà materiali
Corpo base:
	Cu-ETP R300 (EN 13601), tinned

corrosion-resistant, also in aggressive environments

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Cod. art.
01224000