Text for specification

Descrizione
QUADRON®Panel
Base per fusibili NH 400 A, per pannello
vite M10 a entrambi lati
Gr. NH 2 / 3P, con protezione

Norme
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Valori elettrici
corrente nominale (IEC):	400 A
tensione nominale (IEC) AC:	690 V
tensione nominale (IEC) DC:	440 V

power dissipation at full load of the item:	36,0 W
tensione di picco Uimp:	6 kV
tensione max. ammissibile (IEC) AC:	800 V
tensione max. ammissibile (IEC) DC:	800 V
resistenza al corto circuito con protezione tramite fusibili:	50 kA

for fuse links IEC 60269-2 / DIN VDE 0636-201 size 2 up to 45W power dissipation

Proprietà materiali
Corpo base:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contatti:
	spring-loaded copper contacts, silver plated 
Protezione contro contatto accidentale:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
For safe connection of the leads, the shock protection is split into 6.

Brand 
Woehner or equivalent

Cod. art.
03767000