Text for specification

Descrizione
Barra flessibile, isolata
6x 15.5 x 0.8
350 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2011

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	350 A

power dissipation at full load of the item:	69,4 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Cod. art.
01035000