Text for specification

Descrizione
Barra flessibile, isolata
4x 15.5 x 0.8
279 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2020

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	279 A

power dissipation at full load of the item:	66,1 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Cod. art.
01196000