Text for specification

Descrizione
Barra flessibile, isolata
4x 24 x 1
438 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2011

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	438 A

power dissipation at full load of the item:	84,2 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Cod. art.
01253000