Text for specification

Descrizione
CRITO^®60Classic
Piastra con morsetti di connessione, 3 poli
95 -  300 mm²
60Classic

Norme
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Valori elettrici
corrente nominale (IEC):	500 A
tensione nominale (IEC) AC:	690 V
corrente d'impiego max. (IEC):	560 A
tensione max. ammissibile (IEC) AC:	1000 V
tensione max. ammissibile (IEC) DC:	1500 V

resistenza nom. alla corrente di picco I_pk max.:	63,1 kA

Connessioni
for applications acc. to IEC / EN :
Cu 95 - 300 mm² stranded round cables and stranded sectored cables as well as flexible cables (directly)
Cu 240 - 300 mm² fine stranded flexible cables (directly)
Al 120 - 300 mm² stranded round cables and stranded sectored cables
Al 120 - 240 mm² solid sectored cables

for applications acc. to UL / CSA :
Cu 95 - 300 mm² / AWG 3/0 - MCM 600

Suitable for aluminium cables.
When using aluminium cables, observe the maintenance instructions.

Miscellaneous 
Terminals with captive clamping screws
Conductor can be overlapped
Indication of nominal cross-section and tightening torque noted on the terminals.

Brand 
Woehner or equivalent

Cod. art.
01754000