Text for specification

Descrizione
EQUES®185Power
Adattatore 800 A
300 x 652, coll.al sistema in alto / basso, mont.su barre forate
185Power

The 185Power is an innovative busbar system for energy distribution coming with busbar system, connection rails and modules as feeders, busbar connectors, NH in-line fuse-switch-disconnectors, NH switch-disconnector-fuses and adapters for circuit breakers.

 By using Crosslink touch-safe protection modules, it is possible to build a touch-protected 185mm busbar system.

 Crosslink touch-safe protection cover with protection class IP2X front.
 Crosslink touch-safe protection cover with additional front cover enhance protection class to IP4X front.

 All system components can be mounted safely, easily and quickly on the Crosslink touch-safe protection modules using terminal clamps.

The busbar system comes with copper busbars of 30mm, 40mm, 60mm, 80mm, 100mm, 120mm x 10mm. For selected application set up’s, short circuit capabilities are proven by tests. The achievable maximum ratings are rated peak withstand current Ipk max. 105kA, rated short-time withstand current Icw max. 50kA at 1 second. 

Norme
IEC 61439-1:2020

Omologazioni
UL

Valori elettrici
corrente nominale (IEC):	800 A
tensione nominale (IEC) AC:	690 V
tensione nominale (IEC) DC:	800 V

corrente nominale (UL):	800 A
tensione nominale (UL) AC:	1000 V

power dissipation at full load of the item:	176,0 W

tensione nominale di isolamento Ui AC:	1000 V
tensione di picco Uimp:	12 kV

resistenza nom. alla corrente di picco Ipk max.:	106 kA

Brand 
Woehner or equivalent

Cod. art.
32786000A