Text for specification

Descrizione
CRITO®
Morsetto universale
1.5 - 16 mm², AWG 16 - 6
30Compact 3P
60Classic

Norme
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Omologazioni
CSA, UL

Valori elettrici
Corrente nominale (IEC):	65 A
tensione nominale (IEC) AC:	690 V

corrente nominale (UL):	65 A
tensione nominale (UL) AC:	600 V
Utilizzabile fino a max. (IEC):	180 A
tensione max. ammissibile (IEC) AC:	1000 V
tensione max. ammissibile (IEC) DC:	1500 V

resistenza nom. alla corrente di picco Ipk max.:	30,6 kA

Connessioni
1,5 - 16 mm² / AWG 14 - AWG 6 
cavi flessibili, direttam. o con ferrula, 
cavi rotondi rigidi e multifilari, 
bandelle flessibili 8 x 6 x 0,5

(cavi flessibili con ferrula potrebbero no più entrare, se scelti con sezione max. )

Proprietà materiali
Viti di collegamento:
	screw +/- (PZ2), galvanized, chromized 
Corpo del morsetto:
	steel, galvanized and chromized
Retaining spring:
	corrosion-resistant spring steel

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Cod. art.
01284000