Text for specification

Descrizione
CRITO^®
Morsetto a pinza
lam. Cu. 20x3 ... 32x15
60Classic
100Energy
185mm-System
centre feed unit

Norme
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Omologazioni
UL

Valori elettrici
Corrente nominale (IEC):	500 A
tensione nominale (IEC) AC:	690 V

corrente nominale (UL):	800 A
tensione nominale (UL) AC:	600 V
portata massima di corrente con alimentazione centrale:	750 A
Utilizzabile fino a max. (IEC):	750 A
tensione max. ammissibile (IEC) AC:	1000 V
tensione max. ammissibile (IEC) DC:	1500 V

SCCR:	25 kA

Connessioni
bandelle flessibili da 3 x 20 x 1 a 10 x 24 x 1

Proprietà materiali
Viti di collegamento:
	Set screw M16, Allan key size 8
Corpo del morsetto:
	steel, galvanized and chromized
cable base:
	brass, tin plated

Terminal body: 	galvanised steel, chromited screw: 	hexagonal socket screw M16 x 1.5 (S8), galvanised, chromited

Miscellaneous 
Terminal with captive clamping screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal. Contact between conductor and busbar via contact block.

Brand 
Woehner or equivalent

Cod. art.
01319000