Text for specification

Descrizione
Barra flessibile, isolata
10x 15.5 x 0.8
470 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2011

Omologazioni
UL

Valori elettrici
Corrente nominale (IEC):	470 A

power dissipation at full load of the item:	75,1 W

Proprietà materiali
Insulation:
	temperature withstand up to 105 °C
	self-extinguishing, V0 according to UL 94
	breakdown voltage 20 kV
	stretching 370 %

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Cod. art.
01583000