Text for specification

Descrizione
CAPUS®Panel
Sezionatore sottocarico, 3 poli
viti M10, manovra rossa
630 A

Norme
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Omologazioni
IEC (CB)

Valori elettrici
Corrente nominale (IEC):	630 A
tensione nominale (IEC) AC:	500 V

AC-23B (500V)
AC-22B (500V)
AC-21B (500V)

power dissipation at full load of the item:	127,0 W

tensione nominale di isolamento Ui AC:	1000 V
tensione di picco Uimp:	12 kV
potere nominale di chiusura:	30 kA

Switching capacity/utilisation categories AC-23B (500V);  AC-22B (500V); AC-21B (500V)
Mechanical lifespan (switching operations) 7000
Rated short-circuit making capacity 30kA

conv. therm. current in housing
630 A, horizontal installation (adjacent poles) encapsulated 504 x 378 x 302 mm
630 A, vertical installation (poles beneath each other) encapsulated 500 x 500 x 300 mm

Shock protection at front with terminal space cover IP40

Connessioni
viti M10 :
C. serr. 25 - 31 Nm

Miscellaneous 
double-breaking main contacts, 
visible separation sections, 
user-independent switching, 
assembly and connection material contained in scope of delivery

Brand 
Woehner or equivalent

Cod. art.
33357000