Text for specification

Descrizione
Barra flessibile, rame stagnato, isolata
10x 63 x 1
1481 A, lunghezza 2 m
Come accessorio

Norme
IEC 61439-1:2011

Omologazioni
UL

Valori elettrici
Corrente nominale (IEC):	1.481 A

power dissipation at full load of the item:	146,7 W

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Cod. art.
01123000