Text for specification

Descrizione
barra con profilo a TCC, 1600 mm²
lunghezza 2400 mm, stagnata
60Classic
185mm-System
centre feed unit

Norme
IEC 61439-1:2011

Valori elettrici
power dissipation at full load of the item:	251,0 W

diagram current capacity (IEC) 

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Cod. art.
01610000