Text for specification

Descrizione
CRITO®CrossBoard
modulo di connessione
con chiusura a scatto 1,5 - 16 mm², AWG 14 - 6
3p

Norme
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Omologazioni
IEC (CB), UL

Valori elettrici
Corrente nominale (IEC):	63 A
tensione nominale (IEC) AC:	690 V

corrente nominale (UL):	48 A
tensione nominale (UL) AC:	600 V

power dissipation at full load of the item:	4,6 W
Utilizzabile fino a max. (IEC):	80 A

tensione nominale di isolamento Ui AC:	800 V
tensione max. ammissibile (IEC) AC:	800 V
tensione max. ammissibile (IEC) DC:	800 V

resistenza nom. alla corrente di picco Ipk max.:	10 kA

Connessioni
For leads per IEC :
1.5 - 16 mm² round stranded and finely stranded without wire-end ferrule
1.5 - 16 mm² finely stranded with wire-end ferrule*
1.5 - 10 mm² finely stranded with wire-end ferrule 
1.5 - 10 mm² round solid 

* Recommendation: 16 mm² crimped with Rittal crimping pliers for wire-end ferrules WM-Crimp, Weidmüller crimping tool PZ 16 or Phoenix Contact crimping pliers Crimpfox 25R

for leads per UL:
Cu AWG 14 - 6
Class B (UL486E)

Proprietà materiali
Corpo base:
	temperature stability 125°C,
	self-extinguishing in acc. to UL 94,
	creepage resistance CTI 600,
	halogen-free

Brand 
Woehner or equivalent

Cod. art.
01592000A