Text for specification

Description
barramento em perfil duplo T 500 mm²
comprimento 453 mm, estanhado
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
power dissipation at full load of the item:	30,2 W

diagram current capacity (IEC) 

Material properties
Main body:
	Cu-ETP R300 (EN 13601), tinned

corrosion-resistant, also in aggressive environments

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Nº da peça
01225000