Text for specification

Description
CRITO®
terminal condutor universal
1.5 - 16 mm², AWG 16 - 6
30Compact 3P
60Classic
185mm-System

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
CSA, UL

Electrical data
Corrente de medição (IEC):	65 A
Tensão de medição (IEC) AC:	800 V

rated current (UL):	65 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	180 A
tensão máxima IEC AC:	1000 V
tensão máxima IEC DC:	1500 V

rated peak withstand current  Ipk max.:	30,6 kA

pontos terminais
1.5 - 16 mm² / AWG 14 - AWG 6 
flexible cables, directly or with wire-end ferrule, 
solid and stranded round cables, 
lam. Cu 8 x 6 x 0.5

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Material properties
Connecting screws:
	screw +/- (PZ2), galvanized, chromized 
Terminal body:
	steel, galvanized and chromized
Retaining spring:
	corrosion-resistant spring steel

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Nº da peça
01289000