Text for specification

Description
CRITO^®
terminal de pinças
lam. Cu. 20x3 ... 32x15
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Corrente de medição (IEC):	500 A
Tensão de medição (IEC) AC:	690 V

rated current (UL):	800 A
rated voltage (UL) AC:	600 V
Corrente admissível com alimentação central:	750 A
current capacity (IEC) max.:	750 A
tensão máxima IEC AC:	1000 V
tensão máxima IEC DC:	1500 V

SCCR:	25 kA

pontos terminais
lam. Cu from 3 x 20 x 1 to 10 x 24 x 1

Material properties
Connecting screws:
	Set screw M16, Allan key size 8
Terminal body:
	steel, galvanized and chromized
cable base:
	brass, tin plated

Terminal body: 	galvanised steel, chromited screw: 	hexagonal socket screw M16 x 1.5 (S8), galvanised, chromited

Miscellaneous 
Terminal with captive clamping screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal. Contact between conductor and busbar via contact block.

Brand 
Woehner or equivalent

Nº da peça
01319000