Text for specification

Description
CRITO®30Compact
módulo de conexão
com terminais de conexão por mola integrados de 1,5 - 16 mm², AWG 14 - 6
3 polos
30Compact 3P

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Corrente de medição (IEC):	63 A
Tensão de medição (IEC) AC:	690 V

corrente nominal (UL):	48 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	80 A

Tensão nominal de isolamento:	800 V
tensão máxima IEC AC:	800 V
tensão máxima IEC DC:	800 V

rated peak withstand current  Ipk max.:	10 kA

SCCR: 50 kA with JDDZ fuse Class J 60 A / 600 V AC, 35 kA with any DIVQ/7 circuit breaker 60 A / 480 V AC  

pontos terminais
for leads as per IEC :
Cu 1.5 - 16mm²
round conductor solid or stranded, flexible, direct or with wire-end ferrule

for leads as per UL :
Cu AWG 16 - 6
Class B (UL486E)

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Handle:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Brand 
Woehner or equivalent

Nº da peça
01562000A