Text for specification

Description
barramento de cobre laminado, nu, isolado
8x 50 x 1
1114 A, comprimento de 2 m
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Corrente de medição (IEC):	1.114 A

power dissipation at full load of the item:	130,7 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Nº da peça
01343000