Text for specification

Description
módulo N
terminal 16 mm²
9 x 160
30Compact 5P

Standards
IEC 61439-1:2011

Electrical data
Tensão de medição (IEC) AC:	690 V

power dissipation at full load of the item:	0,8 W

Tensão nominal de isolamento:	690 V

Connecting terminal 1.5 - 16mm²

Miscellaneous 
The device can be locked onto the busbar system in a separating position. In this way, complete units 1P+N or 3P+N can be prepared for an isolation test without the leads having to be disconnected. (see assembly manual)

Brand 
Woehner or equivalent

Nº da peça
32632000