Text for specification

Description
QUADRON^®Panel
base fusível NH 160 A
ambos os lados parafusos M8
tamanho 00 / 1P, com proteção contra toque

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Electrical data
Corrente de medição (IEC):	160 A
Tensão de medição (IEC) AC:	690 V
Tensão de medição (IEC) DC:	440 V

power dissipation at full load of the item:	4,2 W
Tensão suportável nominal de impulso Uimp:	6 kV
tensão máxima IEC AC:	1000 V
tensão máxima IEC DC:	1000 V
short-circuit strength when protected by fuses:	50 kA

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contacts:
	spring-loaded copper contacts, silver plated 
Shock protection cover:
	temperature stability 125°C,
	 self-extinguishing in acc. to UL 94,
	 creepage resistance CTI 600,
	 halogen-free 

Miscellaneous 
For safe connection of the leads, the shock protection is split into 2.

Brand 
Woehner or equivalent

Nº da peça
03758000