Text for specification

Description
barramento de cobre laminado, estanhado, isolado
5x 24 x 1
494 A, comprimento de 2 m
Accessories

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
Corrente de medição (IEC):	494 A

power dissipation at full load of the item:	85,7 W

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Nº da peça
01075000