Text for specification

Description
QUADRON®60Classic
base fusível NH 160 A
prensa-cabo
tamanho 00 / 3P
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Approvals
IEC (CB), VDE, CCC

Electrical data
Corrente de medição (IEC):	160 A
Tensão de medição (IEC) AC:	690 V
Tensão de medição (IEC) DC:	440 V

power dissipation at full load of the item:	13,0 W
Tensão suportável nominal de impulso Uimp:	6 kV
tensão máxima IEC AC:	800 V
tensão máxima IEC DC:	800 V
short-circuit strength when protected by fuses:	50 kA

Adapter module: front side degree of protection IP20 as per DIN EN 60529 (finger-safe)

pontos terminais
Box terminal:
1.5 - 70 mm² flexible cables, directly or with wire-end ferrules*, depending on contour of the lead 95 mm² could be connectable 
1.5 - 10 mm² solid round
16 - 70 mm² stranded round 
2x 10 mm², 2x 16 mm² and 2x 25 mm² flexible with wire-end ferrules, identical cables placed side by side, crimping square 
2x 10 - 35 mm² flexible identical cables placed side by side

lam. Cu. 9 - 13 mm wide 
terminal space 13 mm x 13 mm

(*flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
CrossLink® adapter technology
Fast and safe conversion of the connection for top or bottom
Simple and safe clicking into place and making contact
Safe connection through shock protection split into two
Busbar supports for flat busbars can be mounted above each other

Brand 
Woehner or equivalent

Nº da peça
03199000