Text for specification

Description
MOTUS^®30Compact
partida híbrida de motor, 3 polos
partida direta e reversa 1,5 - 7,0 A / interruptor para cargas resistivas 1,5 - 9,0 A
com interface IO-Link
30Compact 3P

Standards
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-2:2011
IEC 61508-1:2010
ISO 13849-1:2015

Approvals
UL

Electrical data
Corrente de medição (IEC):	9 A
Tensão de medição (IEC) AC:	500 V

rated current (UL):	7,6 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	12,0 W

Tensão nominal de isolamento:	550 V
Tensão suportável nominal de impulso Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 175 A / 600 V AC  

pontos terminais
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Nº da peça
36127000A