Text for specification

Description
CRITO®CrossBoard
módulo de conexão
com terminais de conexão por mola integrados de 1,5 - 16 mm², AWG 14 - 6
3 polos

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
IEC (CB), UL

Electrical data
Corrente de medição (IEC):	63 A
Tensão de medição (IEC) AC:	690 V

rated current (UL):	48 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	4,6 W
current capacity (IEC) max.:	80 A

Tensão nominal de isolamento:	800 V
tensão máxima IEC AC:	800 V
tensão máxima IEC DC:	800 V

rated peak withstand current  Ipk max.:	10 kA

pontos terminais
For leads per IEC :
1.5 - 16 mm² round stranded and finely stranded without wire-end ferrule
1.5 - 16 mm² finely stranded with wire-end ferrule*
1.5 - 10 mm² finely stranded with wire-end ferrule 
1.5 - 10 mm² round solid 

* Recommendation: 16 mm² crimped with Rittal crimping pliers for wire-end ferrules WM-Crimp, Weidmüller crimping tool PZ 16 or Phoenix Contact crimping pliers Crimpfox 25R

for leads per UL:
Cu AWG 14 - 6
Class B (UL486E)

Material properties
Main body:
	temperature stability 125°C,
	self-extinguishing in acc. to UL 94,
	creepage resistance CTI 600,
	halogen-free

Brand 
Woehner or equivalent

Nº da peça
01592000A