Text for specification

Описание 
CRITO^®60Classic
Подсоединительная клеммная платформа, 3-полюсная
lam. Cu. 20 - 32 x 3 - 15
60Classic

Стандарты
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Электрические данные
Номинальный ток (IEC):	550 A
номинальное напряжение (IEC) AC:	690 В
токовая нагрузка (IEC) макс.:	800 A
макс. напряжение IEC AC:	1000 В
макс. напряжение IEC DC:	1500 В

номинальный выдерживаемый пиковый ток I  _pk  макс.:	63,1 кА

Особенности клеммной техники
lam. Cu from 3 x 20 x 1 to 10 x 32 x 1

Свойства материала
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free
Cover:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Terminals: 	galvanised steel, chromited screw: 	hexagon socket screw, galvanised, chromited, thrust piece 	brass, nickel-plated

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Арт.
01753000