Text for specification

Описание 
QUADRON®60Classic
Держатель NH предохранителей для монтажа на шины, 250 A
Винт, крепление к шине болтом
Типоразмер 1 / 1 полюс
100Energy
185mm-System

Стандарты
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Электрические данные
Номинальный ток (IEC):	250 A
номинальное напряжение (IEC) AC:	690 В
номинальное напряжение (IEC) DC:	440 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	7,3 Вт
номинальное импульсное напряжение U  imp :	6 kV
макс. напряжение IEC AC:	800 В
макс. напряжение IEC DC:	800 В
устойчивость к короткому замыканию при защите предохранителями:	50 кА

1000V DC, air and creepage distances to DIN EN 60664-1, VDE 0110 Part 1 are to be consideredfor fuse links IEC 60269-2 / DIN VDE 0636-201 size 1 to 32W power dissipation

Свойства материала
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contacts:
	spring-loaded copper contacts, silver plated 
Connecting screws:
	screw M10, galvanized, chromized

Brand 
Woehner or equivalent

Арт.
03601000