Text for specification

Описание 
SECUR^®Panel
Выключатель-разъединитель для D0-предохранителей до 63 А
С LED
1-полюсный

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
VDE

Электрические данные
Номинальный ток (IEC):	63 A
номинальное напряжение (IEC) AC:	400 В
номинальное напряжение (IEC) DC:	65 В

AC-22B (400V)

 DC-22B (65 V)

рассеиваемая мощность при номинальном непрерывном токе устройства:	2,6 Вт

номинальное напряжение изоляции U  _i  AC:	500 В
номинальное импульсное напряжение U  _imp :	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638: AC-22 (400V)

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

There is a transfer of the potential from the busbars, through the LED units, to the terminals  when the fuse links are removed and the switching mechanismn is closed. 

Miscellaneous 
Double function terminal
any feed direction
captive fuse-carrier
sealable operation

Brand 
Woehner or equivalent

Арт.
31556000A