Text for specification

Описание 
CAPUS^®Panel
выключатель-разъединитель нагрузки 3-полюсный
Винт M10, ручка серая
400 A

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
IEC (CB)

Электрические данные
Номинальный ток (IEC):	400 A
номинальное напряжение (IEC) AC:	500 В

AC-23B (500V)
AC-22B (500V)
AC-21B (500V)

рассеиваемая мощность при номинальном непрерывном токе устройства:	57,0 Вт

номинальное напряжение изоляции U  _i  AC:	1000 В
номинальное импульсное напряжение U  _imp :	12 kV
номинальная включающая способность:	30 кА

Mechanical lifespan (switching operations) 7000, rated short-circuit making capacity 30kA

conv. therm. current in housing
400A, horizontal installation (adjacent poles) encapsulated 504 x 378 x 302mm
400A, vertical installation (poles beneath each other) encapsulated 500 x 500 x 300mm

Shock protection at front with terminal space cover IP40

Особенности клеммной техники
screw M10 :
Md 25 - 31 Nm

Miscellaneous 
double-breaking main contacts, visible separation sections, voltage-free exchange of fuses, user-independent switching, assembly and connection material contained in scope of delivery.

Brand 
Woehner or equivalent

Арт.
33334000