Text for specification

Описание 
CRITO®
Универсальная клемма
16 - 120 mm², AWG 6 - 250 MCM
30Compact 3P
60Classic
100Energy
185mm-System
Центральный ввод питания

Стандарты
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Сертификация
CSA, UL

Электрические данные
Номинальный ток (IEC):	250 A
номинальное напряжение (IEC) AC:	800 В

номинальный ток (UL):	255 A
номинальное напряжение (UL) AC:	600 В
токовая нагрузка (IEC) макс.:	440 A
макс. напряжение IEC AC:	1000 В
макс. напряжение IEC DC:	1500 В

номинальный выдерживаемый пиковый ток I  pk  макс.:	62,8 кА

Особенности клеммной техники
16 - 120 mm² / AWG 4 - MCM 250 
flexible cables, directly or with wire-end ferrule, 
solid round cables, 
lam. Cu 4 x 15.5 x 0,8 or 6 x 15.5 x 0,8 or 10 x 15.5 x 0,8

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Арт.
01203000