Text for specification

Описание 
SECUR®Panel
Выключатель-разъединитель для D0-предохранителей до 63 А
3-полюсный

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
VDE, CCC

Электрические данные
Номинальный ток (IEC):	63 A
номинальное напряжение (IEC) AC:	400 В
номинальное напряжение (IEC) DC:	130 В

AC-22B

рассеиваемая мощность при номинальном непрерывном токе устройства:	7,8 Вт

номинальное напряжение изоляции U  i  AC:	500 В
номинальное импульсное напряжение U  imp :	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638 : AC-22

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard. 

Особенности клеммной техники
box terminal :
1,5 - 35 mm²    flexible cables, directly or with wire-end ferrule
(flexible cables of maximum cross-section may not fit when using wire-end ferrule)
1,5 - 10 mm²    solid
Md 2,5 - 3 Nm

2 cables can be connected, when both chambers of the terminal are used
the maximum combination is 35mm² + 16mm²

Miscellaneous 
Double function terminal
any feed direction
captive fuse-carrier
sealable operation

Brand 
Woehner or equivalent

Арт.
31314000A